|  |  |
| --- | --- |
| Affecting Model# | VMAX IP 8CH & 16Ch (Bay Alarm Version) |
| Current Version |  |
| Released Date | 10/7/2016 |
| Announce to | Internal |

|  |  |
| --- | --- |
| Note | 1. Supports Motion Recording for second generation Megapixel Cameras   * DWC-MF21M28T * DWC-MF21M4TIR * DWC-MF21M8TIR * DWC-MD421TIR * DWC-MD421D * DWC-MV421TIR * DWC-MV421D * DWC-MB721M4TIR * DWC-MB721M8TIR * DWC-MB421TIR * DWC-MV82WiA |

Enhancements / Changes/ Fixes

|  |  |
| --- | --- |
| Ref# | Description |
| 001 | 1. Supports Motion Recording for second generation Megapixel Cameras |
| 002 | 1. Second Generation Megapixel Camera Function Matrix with VMAX IP 8&16CH (Bay Alarm version)  - NVR 8CH & 16CH DVR SETUP   1. CAMERA SETUP     2) CAMERA ADVANCED SETUP      3) STREAM SETUP      - NVR 8CH & 16CH WEB REMOTE SETUP  1) CAMERA SETUP    2) CAMERA ADVANCED SETUP    3)STREAM SETUP    O = Supported  X = Not Supported |

Firmware Location

|  |  |
| --- | --- |
| BAY ALARM VER 8CH and 16CH | [VMAX IP 8 & 16CH FW](ftp://47.180.64.250/nvr4ch/INR_ALL_20161004_2334_5_29_0_1_85_Boot.pkg) |
| Login INFO | Username : dw Password : dw1234 |

Special Instruction/Comment

|  |
| --- |
| Following features will be available after second phase developing.   * NVR CAMERA ADVANCED SETUP * WEB REMOTE MOTION MASK SETTING * WEB REMOTE CAMERA ADVANCED SETUP |