|  |  |
| --- | --- |
| Affecting Model# | VMAX IP 8CH & 16Ch (Bay Alarm Version) |
| Current Version |  |
| Released Date | 10/7/2016 |
| Announce to  | Internal |

|  |  |
| --- | --- |
| Note | 1. Supports Motion Recording for second generation Megapixel Cameras* DWC-MF21M28T
* DWC-MF21M4TIR
* DWC-MF21M8TIR
* DWC-MD421TIR
* DWC-MD421D
* DWC-MV421TIR
* DWC-MV421D
* DWC-MB721M4TIR
* DWC-MB721M8TIR
* DWC-MB421TIR
* DWC-MV82WiA
 |

Enhancements / Changes/ Fixes

|  |  |
| --- | --- |
| Ref# | Description |
| 001 | 1. Supports Motion Recording for second generation Megapixel Cameras |
| 002 | 1. Second Generation Megapixel Camera Function Matrix with VMAX IP 8&16CH (Bay Alarm version)- NVR 8CH & 16CH DVR SETUP1. CAMERA SETUP

 2) CAMERA ADVANCED SETUP 3) STREAM SETUP  - NVR 8CH & 16CH WEB REMOTE SETUP 1) CAMERA SETUP 2) CAMERA ADVANCED SETUP  3)STREAM SETUP O = SupportedX = Not Supported  |

Firmware Location

|  |  |
| --- | --- |
| BAY ALARM VER 8CH and 16CH | VMAX IP 8 & 16CH FW |
| Login INFO | Username : dw Password : dw1234 |

Special Instruction/Comment

|  |
| --- |
| Following features will be available after second phase developing.* NVR CAMERA ADVANCED SETUP
* WEB REMOTE MOTION MASK SETTING
* WEB REMOTE CAMERA ADVANCED SETUP
 |